{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["대기오염물질 발생량(연료사용량을 알때)","대기오염물질 발생량(정격가스소비량을 알때)"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"대기오염물질 발생량(연료사용량을 알때)","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["가스열펌프 대기오염물질 발생량 산정내역"]
[]
["○","사업장명 :"]
[]
["○","제조사 / 모델명(대수) :",null,null,"대"]
[{"$nulls":4},"대"]
[{"$nulls":4},"대"]
[{"$nulls":4},"대"]
[{"$nulls":4},"대"]
[{"$nulls":4},"대"]
[]
["○","사용연료종류 :",null,null,"보기"]
[{"$nulls":4},"LPG"]
[{"$nulls":4},"LNG"]
[]
["○","연간연료사용량 :",null,"㎥/년","(LNG)"]
[null,null,null,"kg/년","(LPG)"]
[null,"※ 단위환산계수(대기법 시행규칙 별표10) "]
[null,"   액화천연가스 LNG (1㎏=1.238㎥), 액화석유가스 LPG (1㎏=1.97ℓ=0.529㎥)"]
[]
["○","연간 발생량(LNG) :",{"$f":"C16*(0.03+0.01+3.7)/1000","v":0},"kg/년"]
[null,"- 산출식 : 해당 시설의 연간 연료사용량 x 대기오염물질 배출계수"]
[null,"  배출계수 : 대기환경보전법 시행규칙 별표10(난방분야)"]
[null,"  (먼지 0.03, 황산화물 0.01, 질소산화물 3.70)g/㎥"]
[null,"  연간연료사용량(㎥/년) x (0.03 + 0.01 + 3.70)g/㎥ ÷ 1,000"]
[]
["○","연간 발생량(LPG) :",{"$f":"C17*(0.07+0.01+2.28)/1000","v":0},"kg/년"]
[null,"- 산출식 : 해당 시설의 연간 연료사용량 x 대기오염물질 배출계수"]
[null,"  배출계수 : 대기환경보전법 시행규칙 별표10(난방분야)"]
[null,"  (먼지 0.07, 황산화물 0.01, 질소산화물 2.28)g/kg"]
[null,"  연간연료사용량(kg/년) x (0.07 + 0.01 + 2.28)g/kg ÷ 1,000"]

{"sheet":"대기오염물질 발생량(정격가스소비량을 알때)","index":1,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
["가스열펌프 대기오염물질 발생량 산정내역"]
[]
["○","사업장명 :"]
[]
["○","제조사 / 모델명(대수) :",null,null,"대"]
[{"$nulls":4},"대"]
[{"$nulls":4},"대"]
[{"$nulls":4},"대"]
[{"$nulls":4},"대"]
[{"$nulls":4},"대"]
[]
["○","사용연료종류 :",null,null,"보기"]
[{"$nulls":4},"LPG"]
["○","연간가동시간 :",24,"hr","LNG"]
[null,null,365,"일"]
[null,"- 별도 증빙자료를 제출하는 경우 수정 가능(그외, 24시간 365일 적용)"]
[]
["○","정격가스소비량 :",null,"kw","(LNG)"]
[null,null,null,"kw","(LPG)"]
[]
["○","시간당 가스사용량(LNG) :",{"$f":"C18*860*4.1868/49.4/1000*1.238","v":0},"㎥/hr"]
[null,"- 1kw=860kcal/hr,    1kcal=4.1868kJ"]
[null,"- LNG 순발열량 질량 환산 49.4MJ/kg(에너지법 시행규칙)"]
[null,"※ 단위환산계수(대기법 시행규칙 별표10) "]
[null,"   액화천연가스 LNG (1㎏=1.238㎥), 액화석유가스 LPG (1㎏=1.97ℓ=0.529㎥)"]
[]
["○","시간당 가스사용량(LPG) :",{"$f":"C19*860*4.1868/58.3/1000/0.529","v":0},"kg/hr"]
[null,"- 1kw=860kcal/hr,    1kcal=4.1868kJ"]
[null,"- LPG 순발열량 질량 환산 58.3MJ/kg(에너지법 시행규칙)"]
[null,"※ 단위환산계수(대기법 시행규칙 별표10) "]
[null,"   액화천연가스 LNG (1㎏=1.238㎥), 액화석유가스 LPG (1㎏=1.97ℓ=0.529㎥)"]
[]
["○","연간 발생량(LNG) :",{"$f":"C21*C14*C15*(0.03+0.01+3.7)/1000","v":0},"kg/년"]
[null,"- 산출식 : 시간당 연료사용량 x 일가동시간 x 일가동일수 x 배출계수"]
[null,"  배출계수 : 대기환경보전법 시행규칙 별표10(난방분야)"]
[null,"  (먼지 0.03, 황산화물 0.01, 질소산화물 3.70)g/㎥"]
[]
["○","연간 발생량(LPG) :",{"$f":"C27*C14*C15*(0.07+0.01+2.28)/1000","v":0},"kg/년"]
[null,"- 산출식 : 시간당 연료사용량 x 일가동시간 x 일가동일수 x 배출계수"]
[null,"  배출계수 : 대기환경보전법 시행규칙 별표10(난방분야)"]
[null,"  (먼지 0.07, 황산화물 0.01, 질소산화물 2.28)g/kg"]