{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["원가계산서","내역서총괄표","내역서"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"원가계산서","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[[2,1,2,3],[0,1,1,7]],"flags":["formulas_cached_only"]}
[null,"원가계산서"]
[]
[null,"비            목",null,null,"구분","금    액","요율","산   출   근   거"]
[null,"","재","직   접   재   료   비","1",null,"",""]
[null,"","료","간   접   재   료   비","2",null,"",""]
[null,"","비","작업설.부산물등(△)","3",null,"",""]
[null,"","","소                  계","A",null,"","(1 + 2 + 3 )"]
[null," ","노","직   접   노   무   비","4",null,"",""]
[null,"순","무","간   접   노   무   비","5",null,"13.7%","4 × 0.137"]
[null," ","비","소                  계","B",null,"","( 4 + 5 )"]
[null,"공","","산     출     경    비","6",null,"",""]
[null," ","","산   재   보   험   료","7",null,"3.7%","B × 0.037"]
[null,"사","","고   용   보   험   료","8",null,"1.01%","B × 0.0101"]
[null," ","경","건   강   보   험   료","9",null,"3.495%","4 × 0.03495"]
[null,"원","","연   금   보   험   료","10",null,"4.5%","4 × 0.045"]
[null,"",""," 노인장기요양 보험료","11",null,"12.27%","9 × 0.1227"]
[null,"가",""," 퇴 직 공 제 부 금 비","12",null,"0%","4 × 0.0"]
[null,"","","건설기계대여금지급보증서발급액","13",null,"0.51%","(A + 4 + 6) × 0.0051"]
[null,"","","산 업 안 전 보건관리비","14",null,"2.93%","(A + 4) × 0.0293 × 1.2"]
[null,"","","산 업 안 전 보건관리비","",null,"2.93%","((A + 4) + J/1.1) × 0.0293"]
[null,"","","환   경   보   전   비","15",null,"0.5%","(A + 4 + 6) ×0.005"]
[null,"","","공 사 이 행 보증수수료","16",null,"",""]
[null,"","비","하도급대금지급보증수수료","17",null,"0%","(A + 4 + 6) ×0.0"]
[null,"","","기     타     경    비","18",null,"8.4%","(A + B) × 0.084"]
[null,"","","소                  계","C",null,"","(6:18)"]
[null,"","","순   공  사    원   가","D",null,"","(A + B + C)"]
[null,"","","일   반   관   리   비","E",null,"6%","D × 0.06"]
[null,"","","이                  윤","F",null,"14.965%","(B + C + E) × 0.14965"]
[null,"","","총        원        가","G",null,"","(D + E + F)"]
[null,"","","부   가   가   치   세","H",null,"10%","G × 0.1"]
[null,"","","도        급        액","I",null,"","(G + H)"]
[null,"","","도 급 자 관 급 자 재 대","J",null,"",""]
[null,"","","관 급 자 관 급 자 재 대","K",null,"",""]
[null,"","","총     공    사     비","L",null,"","(I + J + K)"]

{"sheet":"내역서총괄표","index":1,"n_rows":60,"n_cols":11,"rows_kept":60,"cut":false,"hidden":false,"merged":[[0,1,1,10]],"flags":["formulas_cached_only"]}
[null,"내역서총괄표"]
[]
[null,"공종","품    명","규   격","수 량","단위","합    계","노무비","재료비","경    비","비    고"]
[null,"","순 공 사 비","",null,"",null,0,0,0,""]
[null,"A.","다사랑아파트","",null,"",null,0,0,0,""]
[null,"1.","토공","",null,"",null,0,0,0,""]
[null,"1.01.","기존구조물깨기","",null,"",null,0,0,0,""]
[null,"1.02.","터파기","백호(0.4㎥)90%+인력10%",413,"㎥",null,0,0,0,"단산8참조"]
[null,"1.03.","되메우기및다짐(콤팩터)","백호(0.4㎥)90%+인력10%",249,"㎥",null,0,0,0,"단산9참조"]
[null,"1.04.","사토운반","L=15.0km",136,"㎥",null,0,0,0,"단산10참조"]
[null,"1.05.","석분부설","",120,"㎥",null,0,0,0,"단산11참조"]
[null,"1.06.","물푸기","펌프(150mm)+발전기",49,"hr",null,0,0,0,"단산12참조"]
[null,"2.","오수공","",null,"",null,0,0,0,""]
[null,"2.01.","오수관로","",null,"",null,0,0,0,""]
[null,"2.02.","오수받이 연결관","",null,"",null,0,0,0,""]
[null,"2.03.","기존관연결","",null,"",null,0,0,0,""]
[null,"2.04.","신설 오수맨홀","",null,"",null,0,0,0,""]
[null,"2.05.","맨홀 관접합","",null,"",null,0,0,0,""]
[null,"2.06.","맨홀 천공","",null,"",null,0,0,0,""]
[null,"2.07.","부대공","",null,"",null,0,0,0,""]
[null,"3.","포장공","",null,"",null,0,0,0,""]
[null,"3.01.","절삭후덧씌우기","",null,"",null,0,0,0,""]
[null,"3.02.","보도블럭","",null,"",null,0,0,0,""]
[null,"4.","부대공","",null,"",null,0,0,0,""]
[null,"4.01.","차선도색","",null,"",null,0,0,0,""]
[null,"4.02.","조립식 간이흙막이","",null,"",null,0,0,0,""]
[null,"4.03.","지장물매달기","",null,"",null,0,0,0,""]
[null,"4.04.","안전시설비","",null,"",null,0,0,0,""]
[null,"4.05.","시험터파기","",null,"",null,0,0,0,""]
[null,"4.06.","중기운반비","",1,"식",null,0,0,0,"단산65참조"]
[null,"B.","사급자재비","",null,"",null,0,0,0,""]
[null,"1.","골재","",null,"",null,0,0,0,""]
[null,"2.","시멘트, 대전","40kg入(포장품)",25,"포",null,0,0,0,""]
[null,"3.","흄관","",null,"",null,0,0,0,""]
[null,"3.","PE다중벽관","",null,"",null,0,0,0,""]
[null,"4.","아스팔트","",null,"",null,0,0,0,""]
[null,"5.","레미콘(대전)","25-21-080",3,"㎥",null,0,0,0,""]
[null,"6.","분기관 연결구","D100",2,"EA",null,0,0,0,""]
[null,"7.","내충격PVC하수관","",null,"",null,0,0,0,""]
[null,"8.","보차도경계석","",null,"",null,0,0,0,""]
[null,"","간접노무비","",13.7,"%",{"$nulls":4},""]
[null,"","산재보험료","",3.7,"%",{"$nulls":4},""]
[null,"","고용보험료","",1.01,"%",{"$nulls":4},""]
[null,"","건강보험료","",3.495,"%",{"$nulls":4},""]
[null,"","연금보험료","",4.5,"%",{"$nulls":4},""]
[null,"","노인장기요양보험료","",12.27,"%",{"$nulls":4},""]
[null,"","퇴직공제부금비","",null,"%",{"$nulls":4},""]
[null,"","건설기계대여금지급보증서발급액","",0.51,"%",{"$nulls":4},""]
[null,"","환경보전비","",0.5,"%",{"$nulls":4},""]
[null,"","하도급대금지급보증수수료","",null,"%",{"$nulls":4},""]
[null,"","기타경비","",8.4,"%",{"$nulls":4},""]
[null,"","순공사원가","",null,"",{"$nulls":4},""]
[null,"","일반관리비","",6,"%",{"$nulls":4},""]
[null,"","이윤","",14.965,"%",{"$nulls":4},""]
[null,"","총원가","",null,"",{"$nulls":4},""]
[null,"","부가가치세","",10,"%",{"$nulls":4},""]
[null,"","도급액","",null,"",{"$nulls":4},""]
[null,"","도급자관급자재대","",null,"",{"$nulls":4},""]
[null,"","관급자관급자재대","",null,"",{"$nulls":4},""]
[null,"","총공사비","",null,"",{"$nulls":4},""]

{"sheet":"내역서","index":2,"n_rows":173,"n_cols":15,"rows_kept":173,"cut":false,"hidden":false,"merged":[[2,6,2,7],[2,8,2,9],[2,10,2,11],[2,12,2,13],[2,14,3,14],[0,1,1,14],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5]],"flags":["formulas_cached_only"]}
[null,"내역서"]
[]
[null,"공종","품    명","규   격","수 량","단위","합    계",null,"노무비",null,"재료비",null,"경    비",null,"비    고"]
[{"$nulls":6},"단  가","금   액","단  가","금   액","단  가","금   액","단  가","금   액"]
[null,"","순 공 사 비","",null,"",{"$nulls":8},""]
[null,"A.","다사랑아파트","",null,"",{"$nulls":8},""]
[null,"1.","토공","",null,"",{"$nulls":8},""]
[null,"1.01.","기존구조물깨기","",null,"",{"$nulls":8},""]
[null,"","무근콘크리트깨기","T=30cm미만(대형브레이커+0.4㎥)",null,"㎥",{"$nulls":8},"단산1참조"]
[null,"","철근콘크리트깨기","T=30cm미만(대형브레이커+0.4㎥)",null,"㎥",{"$nulls":8},"단산2참조"]
[null,"","아스팔트포장깨기","대형브레이커+0.4㎥",null,"㎥",{"$nulls":8},"단산3참조"]
[null,"","아스팔트포장절단","",null,"M",{"$nulls":8},"단산4참조"]
[null,"","콘크리트 구조물절단","",null,"M",{"$nulls":8},"단산5참조"]
[null,"","보도용 블록 인력철거","B-Type",null,"㎡",{"$nulls":8},"단산6참조"]
[null,"","폐기물상차비","",null,"㎥",{"$nulls":8},"단산7참조"]
[null,"1.02.","터파기","백호(0.4㎥)90%+인력10%",null,"㎥",{"$nulls":8},"단산8참조"]
[null,"1.03.","되메우기및다짐(콤팩터)","백호(0.4㎥)90%+인력10%",null,"㎥",{"$nulls":8},"단산9참조"]
[null,"1.04.","사토운반","L=15.0km",null,"㎥",{"$nulls":8},"단산10참조"]
[null,"1.05.","석분부설","",null,"㎥",{"$nulls":8},"단산11참조"]
[null,"1.06.","물푸기","펌프(150mm)+발전기",null,"hr",{"$nulls":8},"단산12참조"]
[null,"","","",null,"",{"$nulls":8},""]
[null,"2.","오수공","",null,"",{"$nulls":8},""]
[null,"2.01.","오수관로","",null,"",{"$nulls":8},""]
[null,"","PE다중벽관 접합및부설","D=300mm, 환봉지지연결구",null,"m",{"$nulls":8},"단산13참조"]
[null,"","PE다중벽관 이형관 접합및부설","D=300mm",null,"개소",{"$nulls":8},"단산14참조"]
[null,"","PE다중벽관 절단","D=300mm",null,"개소",{"$nulls":8},"단산15참조"]
[null,"2.02.","오수받이 연결관","",null,"",{"$nulls":8},""]
[null,"","내충격PVC하수관 이형관접합및부설","D=100mm",null,"개소",{"$nulls":8},"단산16참조"]
[null,"","내충격PVC하수관 절단","D=100mm",null,"개소",{"$nulls":8},"단산17참조"]
[null,"","분기구접합(PE다중벽관)","D=100mm",null,"개소",{"$nulls":8},"단산18참조"]
[null,"2.03.","기존관연결","",null,"",{"$nulls":8},""]
[null,"","흄관 PE수밀벨트 이형관 접합및부설","D=300mm",null,"개소",{"$nulls":8},"단산19참조"]
[null,"","흄관 절단","D=300mm",null,"개소",{"$nulls":8},"단산20참조"]
[null,"2.04.","신설 오수맨홀","",null,"",{"$nulls":8},""]
[null,"","조립식PC맨홀설치","D900(하부구체+상판)",null,"EA",{"$nulls":8},"단산21참조"]
[null,"","조립식PC맨홀설치","D900(연직구체)",null,"EA",{"$nulls":8},"단산22참조"]
[null,"","조립식 PC 맨홀 하차비","",null,"Ton",{"$nulls":8},"단산23참조"]
[null,"","레미콘타설(장비사용타설)","무근구조물",null,"㎥",{"$nulls":8},"단산24참조"]
[null,"","원형거푸집","3회",null,"㎡",{"$nulls":8},"단산25참조"]
[null,"","합판거푸집","6회",null,"㎡",{"$nulls":8},"단산26참조"]
[null,"","맨홀뚜껑설치","D648",null,"개소",{"$nulls":8},"단산27참조"]
[null,"","사다리설치","후시공용",null,"EA",{"$nulls":8},"단산28참조"]
[null,"2.05.","맨홀 관접합","",null,"",{"$nulls":8},""]
[null,"","맨홀관접합","D=300mm, T=200mm",null,"개소",{"$nulls":8},"단산29참조"]
[null,"","합판거푸집","6회",null,"㎡",{"$nulls":8},"단산26참조"]
[null,"2.06.","맨홀 천공","",null,"",{"$nulls":8},""]
[null,"","맨홀천공접합","D=300mm, T=200mm",null,"개소",{"$nulls":8},"단산31참조"]
[null,"","합판거푸집","6회",null,"㎡",{"$nulls":8},"단산26참조"]
[null,"2.07.","부대공","",null,"",{"$nulls":8},""]
[null,"","하수관 공기압시험","D=300mm이하",null,"개소",{"$nulls":8},"단산32참조"]
[null,"","CCTV 조사(공사후)","신설관, L=520m/일",null,"m",{"$nulls":8},"단산33참조"]
[null,"","관로표시테이프 설치","",null,"m",{"$nulls":8},"단산35참조"]
[null,"","","",null,"",{"$nulls":8},""]
[null,"3.","포장공","",null,"",{"$nulls":8},""]
[null,"3.01.","절삭후덧씌우기","",null,"",{"$nulls":8},""]
[null,"","절삭후 아스팔트덧씌우기","C-Type",null,"㎡",{"$nulls":8},"단산36참조"]
[null,"","텍코팅(인력식)","아스팔트스프레이어400ℓ",null,"㎡",{"$nulls":8},"단산37참조"]
[null,"","보조기층포설및다짐","인력식 소규모 장비사용 시공",null,"㎥",{"$nulls":8},"단산38참조"]
[null,"","프라임코팅(인력식)","아스팔트스프레이어400ℓ",null,"㎡",{"$nulls":8},"단산39참조"]
[null,"","아스팔트 기층 포설및다짐","소규모포설,t=15cm",null,"㎡",{"$nulls":8},"단산40참조"]
[null,"3.02.","보도블럭","",null,"",{"$nulls":8},""]
[null,"","보도용 블록 설치","B-Type",null,"㎡",{"$nulls":8},"단산41참조"]
[null,"","보조기층포설및다짐","인력식 소규모 장비사용 시공",null,"㎥",{"$nulls":8},"단산38참조"]
[null,"","보차도 및 도로경계블록 철거","B-Type, 300mm미만(폭+높이)",null,"M",{"$nulls":8},"단산42참조"]
[null,"","보차도 및 도로경계블록 설치(직선)","B-Type, 300mm미만(폭+높이)",null,"M",{"$nulls":8},"단산43참조"]
[null,"","보차도 및 도로경계블록 철거","B-Type, 350mm미만(폭+높이)",null,"M",{"$nulls":8},"단산44참조"]
[null,"","보차도 및 도로경계블록 설치(직선)","B-Type, 350mm미만(폭+높이)",null,"M",{"$nulls":8},"단산45참조"]
[null,"","모르타르","1:3",null,"㎥",{"$nulls":8},"단산46참조"]
[null,"","레미콘타설(인력운반타설)","무근구조물",null,"㎥",{"$nulls":8},"단산47참조"]
[null,"","","",null,"",{"$nulls":8},""]
[null,"4.","부대공","",null,"",{"$nulls":8},""]
[null,"4.01.","차선도색","",null,"",{"$nulls":8},""]
[null,"","차선밑그림-운행도로,차량부분통제","실선",null,"㎡",{"$nulls":8},"단산48참조"]
[null,"","차선밑그림-운행도로,차량부분통제","횡단보도,주차장",null,"㎡",{"$nulls":8},"단산49참조"]
[null,"","차선도색(융착식,일반형)-운행도로,차량부분통제","수동식,횡단보도.주차장",null,"㎡",{"$nulls":8},"단산50참조"]
[null,"","차선도색(융착식,일반형)-운행도로,차량부분통제","수동식,황색실선",null,"㎡",{"$nulls":8},"단산51참조"]
[null,"4.02.","조립식 간이흙막이","",null,"",{"$nulls":8},""]
[null,"","조립식 간이흙막이 설치및해체","H=3.0m이하, B=1.50m",null,"M",{"$nulls":8},"단산52참조"]
[null,"","조립식 간이흙막이 설치및해체","H=3.0m이하, B=2.30m",null,"M",{"$nulls":8},"단산53참조"]
[null,"4.03.","지장물매달기","",null,"",{"$nulls":8},""]
[null,"","지장물매달기","D80~400mm",null,"개소",{"$nulls":8},"단산54참조"]
[null,"","지장물매달기","D450~700mm",null,"개소",{"$nulls":8},"단산58참조"]
[null,"4.04.","안전시설비","",null,"",{"$nulls":8},""]
[null,"","교통통제 및 안전처리","",null,"일",{"$nulls":8},"단산59참조"]
[null,"","공사안내표지","900 ×1800",null,"EA",{"$nulls":8},"단산60참조"]
[null,"","공사안내현수막","",null,"EA",{"$nulls":8},"단산61참조"]
[null,"","교통안전시설 설치및철거","PE안전휀스(1.5×0.9)",null,"M",{"$nulls":8},"단산62참조"]
[null,"4.05.","시험터파기","",null,"",{"$nulls":8},""]
[null,"","시험터파기","ASP구간",null,"개소",{"$nulls":8},"단산63참조"]
[null,"","시험터파기","보도블럭구간",null,"개소",{"$nulls":8},"단산64참조"]
[null,"4.06.","중기운반비","",null,"식",{"$nulls":8},"단산65참조"]
[null,"","","",null,"",{"$nulls":8},""]
[null,"B.","사급자재비","",null,"",{"$nulls":8},""]
[null,"1.","골재","",null,"",{"$nulls":8},""]
[null,"","모 래, 대전, 도착도","강모래",null,"㎥",{"$nulls":8},""]
[null,"","석 분, 대전, 도착도","",null,"㎥",{"$nulls":8},""]
[null,"","순환골재, 도착도","보조기층재",null,"㎥",{"$nulls":8},""]
[null,"2.","시멘트, 대전","40kg入(포장품)",null,"포",{"$nulls":8},""]
[null,"3.","흄관","",null,"",{"$nulls":8},""]
[null,"","흄관-단관","D300×1.0m",null,"EA",{"$nulls":8},""]
[null,"","수밀벨트(흄관연결용)","Φ300mm",null,"EA",{"$nulls":8},""]
[null,"3.","PE다중벽관","",null,"",{"$nulls":8},""]
[null,"","PE다중벽관(지수단관)","Φ300",null,"EA",{"$nulls":8},""]
[null,"4.","아스팔트","",null,"",{"$nulls":8},""]
[null,"","아스팔트유제","RSC-4",null,"D/M",{"$nulls":8},""]
[null,"","아스팔트유제","RSC-3",null,"D/M",{"$nulls":8},""]
[null,"5.","레미콘(대전)","25-21-080",null,"㎥",{"$nulls":8},""]
[null,"6.","분기관 연결구","D100",null,"EA",{"$nulls":8},""]
[null,"7.","내충격PVC하수관","",null,"",{"$nulls":8},""]
[null,"","내충격PVC하수관-단관","D100×1.0m",null,"EA",{"$nulls":8},""]
[null,"","내충격PVC하수관-소켓","D100",null,"EA",{"$nulls":8},""]
[null,"8.","보차도경계석","",null,"",{"$nulls":8},""]
[null,"","보차도경계석(화강석)","250*300",null,"개",{"$nulls":8},""]
[null,"","보차도경계석(화강석)","250*100(횡단보도,낮춤석)",null,"개",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"◎","도급자관급자재대","",null,"",{"$nulls":8},""]
[null,"1.","아스콘","",null,"",{"$nulls":8},""]
[null,"","아스콘(표층)","조합공통품목, WC-5, 가열, 3등급",null,"톤",{"$nulls":8},"관급"]
[null,"","순환아스콘(기층)","중앙아스콘, BB-2, 상온, 기층용",null,"톤",{"$nulls":8},"관급"]
[null,"","조달수수료","",null,"%",{"$nulls":8},""]
[null,"2.","PE다중벽관","",null,"",{"$nulls":8},""]
[null,"","PE 다중벽관","Φ300mm",null,"m",{"$nulls":8},"관급"]
[null,"","조달수수료","",null,"%",{"$nulls":8},""]
[null,"3.","환봉지지연결구","",null,"",{"$nulls":8},""]
[null,"","환봉지지연결구","Φ300mm",null,"EA",{"$nulls":8},"관급"]
[null,"","조달수수료","",null,"%",{"$nulls":8},""]
[null,"4.","맨홀","",null,"",{"$nulls":8},""]
[null,"","조립식PC맨홀-상부","Φ900mm×H200",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-상부","Φ900mm×H300",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-상부","Φ900mm×H400",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-연직","Φ900mm×H250",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-연직","Φ900mm×H300",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-하부","Φ900mm×H500",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-하부","Φ900mm×H800",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-하부","Φ900mm×H900",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-하부","Φ900mm×H1000",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-사다리","",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-고무링","Φ900mm",null,"EA",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-접합제","",null,"포",{"$nulls":8},"관급"]
[null,"","조립식PC맨홀-접속볼트","",null,"EA",{"$nulls":8},"관급"]
[null,"","맨홀뚜껑","Φ648, 하수도용",null,"조",{"$nulls":8},"관급"]
[null,"","조달수수료","",null,"%",{"$nulls":8},""]
[null,"5.","보도블럭","",null,"",{"$nulls":8},""]
[null,"","보도블럭","투수블럭",null,"㎡",{"$nulls":8},"관급"]
[null,"","조달수수료","",null,"%",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]
[null,"","","",null,"",{"$nulls":8},""]